Installing Bruker wheels is a bit more difficult.

The wheels need to be installed in the following order to work:

1. ts\_remote\_api-2.0.0-py3-none-any.whl
2. bruker\_nmr\_api-1.3.5-py3-none-any.whl
3. requirements.txt

To install:

cd <TopSpin-installation-folder>/python/examples

python -m pip install ts\_remote\_api-2.0.0-py3-none-any.whl

python -m pip install bruker\_nmr\_api-1.3.5-py3-none-any.whl

python -m pip install -r requirements.txt